Environmental Protection Agency

40 CFR Parts 280 and 281 –

**Federal Register** / Vol. 80, No. 135 / Wednesday, July 15, 2015 / Rules and Regulations

Revising Underground Storage Tank Regulations

**Subpart D—Release Detection**

**§ 280.40 General requirements for all UST systems.**

(3) Beginning on October 13, 2018, is operated and maintained, and electronic

and mechanical components are tested for proper operation,

Subpart E—Release Reporting,

Investigation, and Confirmation

*§ 280.50 Reporting of suspected releases*. Owners and operators of UST systems

must report to the implementing agency within 24 hours, or another reasonable

period specified by the implementing agency, and follow the procedures in

§ 280.52 for any of the following conditions:

**(2) Any defective system equipment or component is immediately repaired**

**Or replaced;**

**Full Definition of *DEFECTIVE***

*a* **:**  imperfect in form or function **:**  faulty

*b* **:**  falling below the norm in structure or physical function

Compiled by Iron Ox

Reference: http://www.gpo.gov/fdsys/pkg/FR-2015-07-15/pdf/2015-15914.pdf